


Debounce time from a microswitch gamecontroller.= 1 uS



Debounce time from a microswitch with a transistor BC547 .= 1 uS



The Looptime for the Arduino program = 1,2 mS



The time between a press on the button and the output to the keyboard PC.

Ch1 = output Arduino IO2 / Ch2= input Arduino A0

